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	Comments and Findings include any violations found, clarify all U, N/A and N/C checked: Note: PA Act 287 One Call Law cannot be cited but use 192.614 and company's procedures:

	Item Number
	Qualification
	Comment
	Correct By Date
	Repeat Violation



	Damage Description:
	

	Did the damaged facility have an excess flow valve?
	

	Did Operator notify 911?
	

	Apparent Reason for Damage
	

	Operator Marked Facility with
	

	Operator relationship with Damaging Party
	

	Party Who Damaged is
	

	Municipality
	

	County
	

	Property where damage occurred
	

	Apparent cause of damage
	

	Did the operator follow procedures and regulations regarding repair? (clamp ratings, pre-tested pipe)
	

	Operator's KARL Response
	

	Commodity:
	

	Date of Damage:
	

	Time Of Damage:
	

	Address Of Damage:
	



	Type of Facility Damaged and Size

	Size
	Type Of Facility Damaged

	
	




	Pressure:
	

	Time Notified:
	

	Time Dispatched:
	

	Responder Arrival Time:
	

	Made Safe Time:
	

	Company Response Time:
	

	911 Notified:
	

	Fire Department On-Scene:
	

	Evacuations:
	

	Number Evacuated:
	

	Customers Out of Service:
	

	Number Out of Service:
	

	Isolation Method
	

	One Call Ticket?
	

	Ticket Serial Number:
	

	Facility Marked:
	

	Valid POCS Ticket
	

	Inspection by Operator:
	

	Operator on scene during damage?
	

	Frequency of Inspection
	

	Damaging Party
	

	Party's Address
	

	Contact person:
	

	Telephone:
	

	Type of tool/equipment that caused damage:
	



	Name
	Title
	Phone No

	
	
	



	Regulatory codes
	Compliance Status

	
	



	Latitude:
	

	Longitude:
	



	.605(a)
	Damage Prevention Program Procedure

	
	
	Damage Prevention Program Procedures
	

	
	Damage Prevention Program Procedure

	
	Damage Prevention & Locating

	1.
	Damage Prevention Program Procedure

	
	192.614(c)(1)
	Is the excavator Identified on a listing of those who normally engage in excavating activities?
	

	2.
	Damage Prevention Program Procedure

	
	192.614(c)(2)
	Does the operator's program provide notification to the public and to excavators in the One Call area?
	




	3.
	Damage Prevention Program Procedure

	
	192.614(c)(3)
	Does the damage prevention program provide means for receiving and recording notifications of pending excavations?
	

	4.
	Damage Prevention Program Procedure

	
	192.614(c)(4)
	Does the operator's program provide for notification of pending excavations to the members and how to recognize the temporary markings?
	

	5.
	Damage Prevention Program Procedure

	
	192.614(c)(5)
	Does the program provide means of temporary marking for the pipeline in the vicinity of the excavations as far as practical prior to excavation?
	

	6.
	Damage Prevention Program Procedure

	
	192.614(c)(6)(i)
	Does the program provide for follow-up inspection of the pipeline where there is reason to believe the pipeline could be damaged: Inspection must be done to verify integrity of the pipeline
	

	7.
	Damage Prevention Program Procedure

	
	192.614(c)(6)(ii)
	Does the program specify that a leak survey is mandatory after blasting?
	

	§192.13
	General Pipeline Requirements

	
	§192.13
	What general requirements apply to pipelines regulated under this part?
	

	
	General Pipeline Requirements

	
	§192.13(a)
	No person may operate a segment of pipeline that is readied for service listed in the first column that is readied for service after the date in the second column, unless:
	

	
	§192.13(a)(1)
	The pipeline has been designed, installed, constructed; initially inspected, and initially tested in accordance with this part; or
	

	
	§192.13(a)(2)
	The pipeline qualifies for use under this part according to the requirements in
§192.14.
	

	
	§192.13(a)(2)(i)
	Pipeline
	

	
	§192.13(a)(2)(ii)
	Offshore gathering line.
	

	
	§192.13(a)(2)(iii)
	Regulated onshore gathering line to which this part did not apply until April 14, 2006.
	

	
	§192.13(a)(2)(iv)
	All other pipelines.
	

	
	§192.13(b)
	No person may operate a segment of pipeline listed in the first column that is replaced, relocated, or otherwise changed after the date in the second column, unless that replacement, relocation, or change has been made in accordance with this part.
	

	
	§192.13(b)(i)
	Pipeline
	

	
	§192.13(b)(ii)
	Offshore gathering line.
	

	
	§192.13(b)(iii)
	Regulated onshore gathering line to which this part did not apply until April 14, 2006.
	

	
	§192.13(b)(iv)
	All other pipelines.
	

	
	§192.13(c)
	Each operator shall maintain, modify as appropriate, and follow the plans, procedures, and programs that it is required to establish under this part.
	

	1.
	Inspection Details

	
	§192.614(a)
	Has the operator followed all aspects of their Damage Prevention Program?
	




	2.
	Inspection Details

	
	§59.37
	Is the company's records accurate and current to the conditions found at the time of the mark out showing the size and location of every main, service, valve, drip, district station and other information?
	

	3.
	Inspection Details

	
	§192.603(a)
	Has the operator followed all the provisions of Subpart L?
	

	4.
	Inspection Details

	
	§192.603(b)
	Has the operator kept records of all the provisions of the operations, maintenance, and emergency response manual?
	

	5.
	Inspection Details

	
	§192.605(a)
	Does the operator have up to date procedures for conducting operations, maintenance, and emergency response?
	

	6.
	Inspection Details

	
	§192.605(b)(1)
	Has the operator followed their written procedures with regard to responding to the notification of the damage and subsequent actions taken throughout the emergency and up to and completion of the repair of the damaged facility?
	

	7.
	Inspection Details

	
	§192.605(b)(3)
	Did the operator furnish the appropriate records and maps for the locate and the subsequent emergency for this damage?
	

	8.
	Inspection Details

	
	§192.605(b)(5)
	Did the operator follow Start up and shutdown procedures with stayed within the MAOP of the pipeline system damaged?
	

	9.
	Inspection Details

	
	§192.605(b)(9)
	Did the operator ensure that personnel were protected against hazards & supply the appropriate PPE during the response requirements of this damage?
	

	10.
	Inspection Details

	
	§192.615(a)(4)
	Did the operator have all the necessary personnel and equipment to adequately control the emergency?
	

	11.
	Inspection Details

	
	§192.615(a)(5)
	Did the operator’s actions during the emergency protect people first then property during this emergency?
	

	12.
	Inspection Details

	
	§192.615(a)(6)
	Did the operator shutdown or reduce pressure in order to minimize hazards to life and property during the emergency?
	

	13.
	Inspection Details

	
	§192.615(a)(7)
	Did the operator make safe the actual or potential hazard to life & property?
	

	14.
	Inspection Details

	
	§192.703(c)
	Was the hazardous leak repaired promptly without undue delay?
	

	
	Inspection Details

	
	EFV Installation, Repair, Testing, and MAOP




	15.
	Inspection Details

	
	§192.383(b)
	On single family residences, if the entire service line was replaced, or the tap was replaced, did the operator install an EFV where the pressure operates above 10 psi year around and conditions are conducive for the operation of the valve? (this includes the "new" or "old" tee providing the installation date is/was after February 12, 2010)
	

	16.
	Inspection Details

	
	§192.383(c)
	Does the operator keep records (count) on how many EFV are installed on an annual basis?
	

	17.
	Inspection Details

	
	§192.321(e)
	If the damaged plastic main or newly installed plastic main is not encased (including "push" windows), is or was there a means of locating the main with tracer wire with another technology? (tracer wire must not be wrapped and be installed with minimal contact to the main)
	

	18.
	Inspection Details

	
	§192.361(g)
	If the damaged plastic service line or newly installed service line is not encased, is or was there a means of locating the pipe?
	

	19.
	Inspection Details

	
	§192.143(a)
	For pipe components (including clamps), was the repair in accordance with the requirements for the MAOP of the pipeline?
	

	20.
	Inspection Details

	
	§192.143(b)
	For metallic pipe components (including clamps, metallic tees, and other metallic fittings), was the repair coated and protected in accordance with the Subpart I corrosion control requirements?
	

	21.
	Inspection Details

	
	§192.503(a)(1)
	If there was a segment of pipe replaced, or a section of pipe shutdown (without maintaining pressure) was pretested pipe used which met the requirements of the MAOP?
	

	22.
	Inspection Details

	
	§192.503(d)
	Did the operator perform a leak test on any non-welded joint at its operating pressure?
	

	23.
	Inspection Details

	
	§192.509(b)
	Except service lines and plastic pipelines, did the operator test the main taken out of service appropriately (LP to at least 10 psi & > LP to 90 psi or more)?
	

	24.
	Inspection Details

	
	§192.619(a)(2)
	Did the operator test any steel or plastic pipeline placed into service to 1.5x the MAOP or 1.1x or 1.25x the MAOP in class 1 & 2 areas?
	

	25.
	Inspection Details

	
	§192.511(c)
	Did the operator test any steel service line operating greater than 40 psi to at least 90 psi or any service line operating above 20% SMYS tested to at least 100psi and held for at least 1 hour?
	

	26.
	Inspection Details

	
	§192.513(c)
	For plastic pipe, was the test pressure 1.5x the MAOP or at least 50 psi (which ever was greater)?
	




	27.
	Inspection Details

	
	§192.517(a)
	For High pressure pipe, does the operator record details of the test and keep the appropriate records for the life of the pipe?
	

	28.
	Inspection Details

	
	§192.517(b)
	For pipelines operating below 100 psi or for service lines and/or plastic pipelines, does the operator keep the records of the pressure test for a minimum of 5 years?
	

	
	Miscellaneous Requirements

	
	
	Damage Response
	

	29.
	Miscellaneous Requirements

	
	59.33
	Did the operator take all reasonable steps to properly warn via locate marks and protect the public from danger, and exercise reasonable care to reduce the hazards to excavators, employees, and the public?
	

	§192.605
	Operations & Maintenance Plan

	
	
	§192.605 Procedural manual for operations, maintenance, and emergencies. Each operator shall include the following in its operating and maintenance plan:
	

	
	Operations & Maintenance Plan

	
	§192.605(a)
	General. Each operator shall prepare and follow for each pipeline, a manual of written procedures for conducting operations and maintenance activities and for emergency response. For transmission lines, the manual must also include procedures for handling abnormal operations. This manual must be reviewed and updated by the operator at intervals not exceeding 15 months, but at least one each calendar year. This manual must be prepared before operations of a pipeline system commence. Appropriate parts of the manual must be kept at locations where operations and maintenance activities are conducted.
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