FOR DISCUSSION PURPOSES ONLY. THIS IS NOT A FULLY PUBLISEHD XML/WSDL SPECIFICATION.

IT IS INTENDED TO DESCRIBE THE DATA PROVIDED.

A FULLY PUBLISHED WSDL WOULD INCLUDE POST, SOAPAction, AND OTHER STANDARD PARAMETERS.

SOAP/WSDL Request (inclusion of a header with credentials is implied):

<soap:Envelope>

<soap:Body>

<EDC\_ACCT\_NO>

<decimal>1111111111</decimal>

</EDC\_ACCT\_NO>

<USAGE\_DATES>

<FROM>20140101</FROM>

<TO>20140102</TO>

</USAGE\_DATES>

<IURequestLevel>

<char>Account OR Meter</char>

</IURequestLevel>

</soap:Body>

</soap:Envelope>

\*\* Comment -- If usage dates are not present in request, EDC will provide all available IU data up to a maximum equal to or greater than the 12 most recent calendar months)

SOAP/WSDL Successful Account-Level IU Response:

<soap:Envelope>

<soap:Body>

<STATUS\_CODE>

<char>0</char>

</STATUS\_CODE>

<STATUS\_MESSAGE>

<char>Successful</char>

</STATUS\_MESSAGE>

<IUAccountLevelResponse>

<arr:IU\_ACCT>

<IU\_ACCT>

<EDC\_ACCT\_NO>

<decimal>1111111111</decimal>

</EDC\_ACCT\_NO>

<USAGE\_DATE>20140101/>

<60MinuteIU>

<IU\_0100>0.917</IU\_0100>

<QTY\_0100>QD</QTY\_0100>

----------------

<IU\_2400>0.947</IU\_2400>

<QTY\_2400>KA</QTY\_2400>

</60MinuteIU>

</IU\_ACCT>

<IU\_ACCT>

<EDC\_ACCT\_NO>

<decimal>1111111111</decimal>

</EDC\_ACCT\_NO>

<USAGE\_DATE>20140102/>

<60MinuteIU>

<IU\_0100>0.738</IU\_0100>

<QTY\_0100>87</QTY\_0100>

----------------

<IU\_2400>0.821</IU\_2400>

<QTY\_2400>QD</QTY\_2400>

</60MinuteIU>

</IU\_ACCT>

</arr:IU\_ACCT>

</IUAccountLevelResponse>

</soap:Body>

</soap:Envelope>

\*\* Comment -- Increments can vary - 60MinuteIU, 30MinuteIU, 15MinuteIU - by EDC.

\*\* Comment -- On Long DST Day only, will include <IU\_0200D> interval

\*\* Comment -- On Short DST Day only, will omit <IU\_0300> interval

SOAP/WSDL Successful Meter-Level IU Response:

<soap:Envelope>

<soap:Body>

<STATUS\_CODE>

<char>0</char>

</STATUS\_CODE>

<STATUS\_MESSAGE>

<char>Successful</char>

</STATUS\_MESSAGE>

<IUMeterLevelResponse>

<EDC\_ACCT\_NO>

<decimal>1111111111</decimal>

</EDC\_ACCT\_NO>

<arr:IU\_METER>

<IU\_METER>

<METER\_NO>12345</METER\_NO>

<METER\_MULTIPLIER>1</METER\_MULTIPLIER>

<USAGE\_DATE>20140101/>

<60MinuteIU>

<IU\_0100>0.917</IU\_0100>

<QTY\_0100>QD</QTY\_0100>

----------------

<IU\_2400>0.947</IU\_2400>

<QTY\_2400>KA</QTY\_2400>

</60MinuteIU>

</IU\_METER>

<IU\_METER>

<METER\_NO>12345</METER\_NO>

<METER\_MULTIPLIER>1</METER\_MULTIPLIER>

<USAGE\_DATE>20140102/>

<60MinuteIU>

<IU\_0100>0.738</IU\_0100>

<QTY\_0100>KA</QTY\_0100>

----------------

<IU\_2400>0.821</IU\_2400>

<QTY\_2400>QD</QTY\_2400>

</60MinuteIU>

</IU\_METER>

----------------

<IU\_METER>

<METER\_NO>54321</METER\_NO>

<METER\_MULTIPLIER>1</METER\_MULTIPLIER>

<USAGE\_DATE>20140101/>

<60MinuteIU>

<IU\_0100>0.3</IU\_0100>

<QTY\_0100>87</QTY\_0100>

----------------

<IU\_2400>0.152</IU\_2400>

<QTY\_2400>9H</QTY\_2400>

</60MinuteIU>

</IU\_METER>

<IU\_METER>

<METER\_NO>54321</METER\_NO>

<METER\_MULTIPLIER>1</METER\_MULTIPLIER>

<USAGE\_DATE>20140102/>

<60MinuteIU>

<IU\_0100>0.738</IU\_0100>

<QTY\_0100>87</QTY\_0100>

----------------

<IU\_2400>0.821</IU\_2400>

<QTY\_2400>87</QTY\_2400>

</60MinuteIU>

</IU\_METER>

</arr:IU\_METER>

</IUMeterLevelResponse>

</soap:Body>

</soap:Envelope>

\*\* Comment -- Increments can vary - 60MinuteIU, 30MinuteIU, 15MinuteIU - by EDC.

\*\* Comment -- On Long DST Day only, will include <IU\_0200D> interval

\*\* Comment -- On Short DST Day only, will omit <IU\_0300> interval

SOAP/WSDL Rejected IU Response: Only status code and message are returned.

<soap:Envelope>

<soap:Body>

<STATUS\_CODE>

<char> ... </char>

</STATUS\_CODE>

<STATUS\_MESSAGE>

<char> ... </char>

</STATUS\_MESSAGE>

</soap:Body>

</soap:Envelope>

\*\* The body of a response indicating rejection of a request will contain either a standard HTTP status code & message, or an existing EDI HI rejection code and associated message.